BL51 BANKED LINKER/LOCATER V6.11                                                        08/17/2013  10:53:06  PAGE 1


BL51 BANKED LINKER/LOCATER V6.11, INVOKED BY:
C:\KEIL\C51\BIN\BL51.EXE keypad_controlled_leds.obj TO keypad_controlled_leds RAMSIZE (256)


MEMORY MODEL: SMALL


INPUT MODULES INCLUDED:
  keypad_controlled_leds.obj (KEYPAD_CONTROLLED_LEDS)
  C:\KEIL\C51\LIB\C51S.LIB (?C_STARTUP)


LINK MAP OF MODULE:  keypad_controlled_leds (KEYPAD_CONTROLLED_LEDS)


            TYPE    BASE      LENGTH    RELOCATION   SEGMENT NAME
            -----------------------------------------------------

            * * * * * * *   D A T A   M E M O R Y   * * * * * * *
            REG     0000H     0008H     ABSOLUTE     "REG BANK 0"
            IDATA   0008H     0001H     UNIT         ?STACK

            * * * * * * *   C O D E   M E M O R Y   * * * * * * *
            CODE    0000H     0003H     ABSOLUTE     
                    0003H     07FDH                  *** GAP ***
            CODE    0800H     0025H     UNIT         ?PR?MAIN?KEYPAD_CONTROLLED_LEDS
            CODE    0825H     0020H     UNIT         ?PR?_DELAY?KEYPAD_CONTROLLED_LEDS
            CODE    0845H     000CH     UNIT         ?C_C51STARTUP



OVERLAY MAP OF MODULE:   keypad_controlled_leds (KEYPAD_CONTROLLED_LEDS)


SEGMENT
  +--> CALLED SEGMENT
---------------------
?C_C51STARTUP
  +--> ?PR?MAIN?KEYPAD_CONTROLLED_LEDS

?PR?MAIN?KEYPAD_CONTROLLED_LEDS
  +--> ?PR?_DELAY?KEYPAD_CONTROLLED_LEDS



SYMBOL TABLE OF MODULE:  keypad_controlled_leds (KEYPAD_CONTROLLED_LEDS)

  VALUE           TYPE          NAME
  ----------------------------------

  -------         MODULE        KEYPAD_CONTROLLED_LEDS
  C:0000H         SYMBOL        _ICE_DUMMY_
  D:0080H         PUBLIC        P0
  D:0090H         PUBLIC        P1
  D:00A0H         PUBLIC        P2
  D:00B0H         PUBLIC        P3
  D:00A8H         PUBLIC        IE
  C:0825H         PUBLIC        _delay
BL51 BANKED LINKER/LOCATER V6.11                                                      08/17/2013  10:53:06  PAGE 2


  D:00B8H         PUBLIC        IP
  C:0800H         PUBLIC        main
  D:0098H         PUBLIC        SCON
  D:0088H         PUBLIC        TCON
  B:0080H.0       PUBLIC        switch1
  B:0080H.1       PUBLIC        switch2
  B:0080H.2       PUBLIC        switch3
  B:0080H.3       PUBLIC        switch4
  B:0080H.4       PUBLIC        switch5
  B:0080H.5       PUBLIC        switch6
  B:0080H.6       PUBLIC        switch7
  B:0080H.7       PUBLIC        switch8
  D:00C8H         PUBLIC        T2CON
  D:00D0H         PUBLIC        PSW
  -------         PROC          MAIN
  C:0800H         LINE#         30
  C:0800H         LINE#         31
  C:0800H         LINE#         32
  C:0802H         LINE#         33
  C:0804H         LINE#         34
  C:0806H         LINE#         35
  C:0808H         LINE#         36
  C:080AH         LINE#         37
  C:080CH         LINE#         38
  C:080EH         LINE#         39
  C:0810H         LINE#         40
  C:0813H         LINE#         41
  C:0813H         LINE#         42
  C:0813H         LINE#         43
  C:0816H         LINE#         44
  C:0816H         LINE#         45
  C:0819H         LINE#         46
  C:0820H         LINE#         47
  C:0823H         LINE#         48
  C:0823H         LINE#         50
  -------         ENDPROC       MAIN
  -------         PROC          _DELAY
  D:0006H         SYMBOL        time
  -------         DO            
  D:0004H         SYMBOL        i
  D:0002H         SYMBOL        j
  -------         ENDDO         
  C:0825H         LINE#         53
  C:0825H         LINE#         54
  C:0825H         LINE#         56
  C:082FH         LINE#         57
  C:0844H         LINE#         58
  -------         ENDPROC       _DELAY
  -------         ENDMOD        KEYPAD_CONTROLLED_LEDS

******************************************************************************
* RESTRICTED VERSION WITH 0800H BYTE CODE SIZE LIMIT; USED: 0045H BYTE ( 3%) *
******************************************************************************

Program Size: data=9.0 xdata=0 code=84
LINK/LOCATE RUN COMPLETE.  0 WARNING(S),  0 ERROR(S)
